# Weather Station Data Summarization and Manipulation for HOBO Data Loggers

## Documentation for package ‘hoboR’ version 1.1.0

- DESCRIPTION file.

## Help Pages

calibrator | Calibrator HOBO data in CSV format
correction | Correction test for HOBO data from calibrator
correction.test | Correction Test for HOBO data from calibrator
count_NAs | HOBO count NA's This function counts the number of NA's in your data set
hobinder | Reads HOBO data in CSV format
hobocleaner | Reads HOBO data in CSV format
hobocorrelations | Correlation plot for variables within a time range
hoborange | Calculate Date Range Temperature Using HOBO Data
hobotime | Summarise HOBO data by time intervals
impossiblevalues | HOBO impossible values
meanhobo | mean HOBO data in CSV format
sampling.rates | Calculates sampling rates from a CSV format
sensorfailures | HOBO Remove Values This function is designed to identify and address values that are likely to be out of range, such as temperatures exceeding the maximum recorded in your study area or relative humidity (RH) values exceeding 100%, which are not feasible. The 'sensorfailure()' function allows you to detect and flag these anomalous readings, facilitating the cleansing of your dataset by replacing all out-of-range values with NA's, maintaining the integrity and accuracy of of your data analysis.
testhobolist | Test HOBO data for calibration
timestamp | Timestamp for Specific Intervals